**This AHA is provided as an example of content to consider during development of project-specific AHAs for like activities**

|  |
| --- |
| **Activity**: Dust particulate isolation  |

|  |
| --- |
| **HAZARDS** |
| *JOB STEP* | *HAZARDS* | *ACTIONS TO ELIMINATE OR MINIMIZE**EACH HAZARD* |
| Lay out area for temporary containment | Risks of damage to property | Ensure all unassociated areas are isolated from dust / particulates originating from construction. |
| Use a chop or circular saw to cut material for temp wall | Risk of injury due to repetitive motion | All employees shall follow good ergonomics and/or reference company ergonomic program.Injuries shall be reported immediately to supervisor.Choose the proper tools for the job. |
| Install temporary wall supports | Risks of bodily injury | Minimum-required PPE worn at all times. Clear work area of clutter. Make sure tools are in proper working condition.  |
| Install poly sheeting | Risks of bodily injury | Minimum-required PPE worn at all times.  |