**This AHA is provided as an example of content to consider during development of project-specific AHAs for like activities**

|  |
| --- |
| **Activity**: Use of laser level following OSHA 1926.54 |

|  |
| --- |
| **HAZARDS** |
| *JOB STEP* | *HAZARDS* | *ACTIONS TO ELIMINATE OR MINIMIZE**EACH HAZARD* |
| Use of laser level  | Risk of exposure to a laser light | Ensure work area is clearly labeled with Signage stating “Laser in Use”.Lasers shall be less than 0.5 wattsOnly necessary personnel in room while laser is operated by qualified personnel only.Laser level will be turned off when not in use.The laser beam shall not be directed at employees.Laser unit in operation should be set up above the heads of the employees when possible. |