**This AHA is provided as an example of content to consider during development of project-specific AHAs for like activities**

|  |
| --- |
| **Activity**: Use pf all-terrain and powered industrial trucks (PIT) following OSHA 1926 Subpart O |

|  |
| --- |
| **HAZARDS** |
| *JOB STEP* | *HAZARDS* | *ACTIONS TO ELIMINATE OR MINIMIZE**EACH HAZARD* |
| Use of an all-terrain or powered industrial trucks: | Risk of injury to automotive or pedestrian traffic. | A traffic / pedestrian plan may be required for this projectIf transporting tools, equipment or material a spotter, escort or certified flaggers will be required. |
| Risk of serious bodily injury or death | Read the manufacture’s manual. Follow manufacturer’s recommendations. Only trained and authorized personal shall operate lifts. A spotter maybe required to assist with traffic and pedestrian control when in travel.Be aware of surroundings.Identify overhead and ground obstructions.Minimum-required PPE worn at all times.  |
| Risk of equipment failure or malfunction | Perform pre-use inspections as per the manufacture’s requirements. Any equipment deemed not safe shall be “RED” tagged and removed from service immediately.Only use designated and manufacturer-approved attachments.Maintain proper load capacity within the stability tri-angle according to the capacity plate. |