**This AHA is provided as an example of content to consider during development of project-specific AHAs for like activities**

|  |
| --- |
| **Activity**:  Use pf all-terrain and powered industrial trucks (PIT) following OSHA 1926 Subpart O |

|  |  |  |
| --- | --- | --- |
| **HAZARDS** | | |
| *JOB STEP* | *HAZARDS* | *ACTIONS TO ELIMINATE OR MINIMIZE*  *EACH HAZARD* |
| Use of an all-terrain or powered industrial trucks: | Risk of injury to automotive or pedestrian traffic. | A traffic / pedestrian plan may be required for this project  If transporting tools, equipment or material a spotter, escort or certified flaggers will be required. |
| Risk of serious bodily injury or death | Read the manufacture’s manual. Follow manufacturer’s recommendations.  Only trained and authorized personal shall operate lifts.  A spotter maybe required to assist with traffic and pedestrian control when in travel.  Be aware of surroundings.  Identify overhead and ground obstructions.  Minimum-required PPE worn at all times. |
| Risk of equipment failure or malfunction | Perform pre-use inspections as per the manufacture’s requirements.  Any equipment deemed not safe shall be “RED” tagged and removed from service immediately.  Only use designated and manufacturer-approved attachments.  Maintain proper load capacity within the stability tri-angle according to the capacity plate. |