**This AHA is provided as an example of content to consider during development of project-specific AHAs for like activities**

|  |
| --- |
| **Activity**: Flooring installation (carpet, sheet vinyl, VCT, tile)  |

|  |
| --- |
| **HAZARDS** |
| *JOB STEP* | *HAZARDS* | *ACTIONS TO ELIMINATE OR MINIMIZE**EACH HAZARD* |
| Floor prep and layout:  | Risk of exposure to asbestos from VCT/ mastic under lament | Reference results of ACM survey. |
| Install flooring | Risk of exposure to silica based products | Respirators or dust masks may be required. Respirator use in accordance with Respiratory Protection Program, including medical evaluation and fit testing. |
| Risk of fire from heat gun or open flamed tool | Follow the Hot Work Permit as required.Fire watch is required (trained in fire extinguishers).Employee shall have proper training on heat guns or open flamed tools. |
| Risk of injuries/ cuts from improper tool use or storage. | Employees are to be trained on the use of tools.Protect knifes or open blade with a holder or sheath to protect the blade while not in use.Keep all used razor blades in a sharps container labeled as "SHARPS” |