**This AHA is provided as an example of content to consider during development of project-specific AHAs for like activities**

|  |
| --- |
| **Activity**: Installing Insulation  |

|  |
| --- |
| **HAZARDS** |
| *JOB STEP* | *HAZARDS* | *ACTIONS TO ELIMINATE OR MINIMIZE**EACH HAZARD* |
| Install insulation | Risk of exposure to fiberglass particles. | Minimum-required PPE worn at all times, including long sleeves and gloves.Respirators or dust masks may be required when drilling into concrete. Respirator use in accordance with Respiratory Protection Program, including medical evaluation and fit testing. |
| Risk of injuries/ cuts from improper tool use or storage. | Employees are to be trained on the use of tools.Protect knifes or open blade with a holder or sheath to protect the blade while not in use.Keep all used razor blades in a sharps container labeled as "SHARPS" |